CONFIG_CNSS_QCA6390 := y
CONFIG_BUS_AUTO_SUSPEND := y
CONFIG_DIRECT_BUF_RX_ENABLE := y
CONFIG_WMI_DBR_SUPPORT := y
CONFIG_TX_AGGREGATION_SIZE_ENABLE := y
CONFIG_RX_PERFORMANCE := y
#Flag to enable pre cac feature
CONFIG_FEATURE_WLAN_PRE_CAC := y

ifeq ($(CONFIG_CNSS_QCA6390), y)
	ifeq ($(CONFIG_CNSS_EMULATION), y)
		CONFIG_QCA_WIFI_NAPIER_EMULATION := y
	endif
	CONFIG_LITHIUM := y
	CONFIG_WLAN_FEATURE_11AX := y
	CONFIG_WLAN_FEATURE_DFS_OFFLOAD := y
	CONFIG_SCALE_INCLUDES := y
	CONFIG_MORE_TX_DESC := y
	CONFIG_FW_THERMAL_THROTTLE := y
	CONFIG_WLAN_FEATURE_MBSSID := y
endif

ifeq ($(CONFIG_ENABLE_IPA), y)
	CONFIG_IPA3 := y
	CONFIG_WDI3_IPA_OVER_GSI := y
else
	ifeq ($(CONFIG_ENABLE_IPA), n)
		CONFIG_IPA3 := n
	endif
endif

ifeq ($(CONFIG_CLD_HL_SDIO_CORE), y)
	CONFIG_QCA_WIFI_SDIO := y
ifndef CONFIG_SDIO_TRANSFER
	CONFIG_SDIO_TRANSFER = mailbox
endif
endif

ifeq ($(CONFIG_QCA_WIFI_SDIO), y)
	CONFIG_ROME_IF = sdio
endif

ifdef CONFIG_ICNSS
	CONFIG_ROME_IF = snoc
endif

ifeq (y,$(findstring y,$(CONFIG_CNSS) $(CONFIG_CNSS2)))
ifndef CONFIG_ROME_IF
	#use pci as default interface
	CONFIG_ROME_IF = pci
endif
endif

ifeq (m,$(findstring m,$(CONFIG_CNSS) $(CONFIG_CNSS2)))
ifndef CONFIG_ROME_IF
	#use pci as default interface
	CONFIG_ROME_IF = pci
endif
endif

# Make WLAN as open-source driver by default
WLAN_OPEN_SOURCE := y

ifeq ($(CONFIG_ICNSS), y)
	CONFIG_HELIUMPLUS := y
	CONFIG_64BIT_PADDR := y
	CONFIG_FEATURE_TSO := y
	CONFIG_FEATURE_TSO_DEBUG := y
	ifeq ($(CONFIG_INET_LRO), y)
		CONFIG_WLAN_LRO := y
	else
		CONFIG_WLAN_LRO := n
	endif
endif

ifneq ($(DEVELOPER_DISABLE_BUILD_TIMESTAMP), y)
ifneq ($(WLAN_DISABLE_BUILD_TAG), y)
CONFIG_BUILD_TAG := y
endif
endif

ifeq ($(CONFIG_ARCH_MDM9630), y)
CONFIG_MOBILE_ROUTER := y
endif

ifeq ($(CONFIG_ARCH_MDM9640), y)
CONFIG_MOBILE_ROUTER := y
endif

ifeq ($(CONFIG_ARCH_SDX20), y)
CONFIG_MOBILE_ROUTER := y
endif

ifeq (y, $(filter y, $(CONFIG_ARCH_SDXPRAIRIE) $(CONFIG_ARCH_SA515) $(CONFIG_ARCH_SDXPOORWILLS)))
CONFIG_MOBILE_ROUTER := y
endif

ifeq ($(CONFIG_ARCH_MSM8917), y)
	ifeq ($(CONFIG_ROME_IF), sdio)
		CONFIG_WLAN_SYNC_TSF_PLUS := y
	endif
endif

ifeq ($(CONFIG_ARCH_QCS405), y)
	CONFIG_WLAN_SYNC_TSF_PLUS := y
	CONFIG_WLAN_SYNC_TSF_PLUS_NOIRQ := y
endif

#Flag to enable Legacy Fast Roaming3(LFR3)
ifeq (y,$(findstring y,$(CONFIG_HELIUMPLUS) $(CONFIG_LITHIUM)))
	CONFIG_QCACLD_WLAN_LFR3 := y
else
	CONFIG_QCACLD_WLAN_LFR2 := y
endif

ifeq ($(CONFIG_LITHIUM), y)
CONFIG_WIFI_MONITOR_SUPPORT := y
CONFIG_QCA_MONITOR_PKT_SUPPORT := y
CONFIG_MONITOR_MODULARIZED_ENABLE := n
endif

ifneq ($(CONFIG_MOBILE_ROUTER), y)
#Flag to enable TDLS feature
CONFIG_QCOM_TDLS := y

CONFIG_WLAN_SYSFS := y
endif

CONFIG_QCACLD_FEATURE_GREEN_AP := y
#Flag to enable Android Packet Filtering
CONFIG_QCACLD_FEATURE_APF := y

#Flag to enable SARv1 -> SARv2 conversion
CONFIG_WLAN_FEATURE_SARV1_TO_SARV2 := n

ifeq ($(CONFIG_ARCH_MSM8998), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

ifeq ($(CONFIG_ARCH_SDM660), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

ifeq ($(CONFIG_ARCH_SDM630), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

ifeq ($(CONFIG_ARCH_SDM845), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

ifeq ($(CONFIG_ARCH_SM8150), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

ifeq ($(CONFIG_ARCH_SDM670), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

ifeq ($(CONFIG_ARCH_SM6150), y)
CONFIG_QCACLD_FEATURE_METERING := y
endif

#Flag to enable Fast Transition (11r) feature
CONFIG_QCOM_VOWIFI_11R := y

#Flag to enable disable ACTION OUI feature
CONFIG_WLAN_FEATURE_ACTION_OUI := y

#Flag to enable FILS Feature (11ai)
CONFIG_WLAN_FEATURE_FILS := y
ifneq ($(CONFIG_QCA_CLD_WLAN),)
	ifeq (y,$(findstring y,$(CONFIG_CNSS) $(CONFIG_CNSS2) $(CONFIG_ICNSS)))
	#Flag to enable LTE CoEx feature
	CONFIG_QCOM_LTE_COEX := y
		ifneq ($(CONFIG_MOBILE_ROUTER), y)
		#Flag to enable LPSS feature
		CONFIG_WLAN_FEATURE_LPSS := y
		endif
	endif

	ifeq (m,$(findstring m,$(CONFIG_CNSS2)))
	#Flag to enable LTE CoEx feature
	CONFIG_QCOM_LTE_COEX := y
		ifneq ($(CONFIG_MOBILE_ROUTER), y)
		#Flag to enable LPSS feature
		CONFIG_WLAN_FEATURE_LPSS := y
		endif
	endif
endif

#Flag to enable the tx desc sanity check
ifeq ($(CONFIG_ROME_IF),usb)
	CONFIG_QCA_TXDESC_SANITY_CHECKS := y
endif

ifneq ($(CONFIG_MOBILE_ROUTER), y)
	#Flag to enable NAN
	CONFIG_QCACLD_FEATURE_NAN := y
	CONFIG_NDP_SAP_CONCURRENCY_ENABLE := y
endif

#Flag to enable Linux QCMBR feature as default feature
ifeq ($(CONFIG_ROME_IF),usb)
	CONFIG_LINUX_QCMBR :=y
endif


CONFIG_FEATURE_EPPING := y

#Flag to enable offload packets feature
CONFIG_WLAN_OFFLOAD_PACKETS := y

#enable TSF get feature
CONFIG_WLAN_SYNC_TSF := y
#Enable DSRC feature
ifeq ($(CONFIG_QCA_WIFI_SDIO), y)
	#Enable DSRC feature
	CONFIG_WLAN_FEATURE_DSRC := y
else
	CONFIG_WLAN_REG_AUTO := y
endif

ifneq ($(CONFIG_ROME_IF),usb)
	#Flag to enable SAE
	CONFIG_WLAN_FEATURE_SAE := y

ifneq ($(CONFIG_ROME_IF),sdio)
	#Flag to enable DISA
	CONFIG_WLAN_FEATURE_DISA := y

	#Flag to enable FIPS
	CONFIG_WLAN_FEATURE_FIPS := y

	#Flag to enable Fast Path feature
	ifneq ($(CONFIG_LITHIUM), y)
		CONFIG_WLAN_FASTPATH := y
	endif

	# Flag to enable NAPI
	CONFIG_WLAN_NAPI := y
	CONFIG_WLAN_NAPI_DEBUG := n

	# Flag to enable FW based TX Flow control
	ifeq ($(CONFIG_LITHIUM), y)
		CONFIG_WLAN_TX_FLOW_CONTROL_V2 := y
	else
		CONFIG_WLAN_TX_FLOW_CONTROL_V2 := n
	endif

endif
endif

CONFIG_POWER_MANAGEMENT_OFFLOAD := y

ifeq ($(CONFIG_ROME_IF), snoc)
	CONFIG_WLAN_TX_FLOW_CONTROL_V2 := y
endif

# Flag to enable LFR Subnet Detection
CONFIG_LFR_SUBNET_DETECTION := y

# Flag to enable MCC to SCC switch feature
CONFIG_MCC_TO_SCC_SWITCH := y

ifeq ($(CONFIG_SLUB_DEBUG), y)
	# Enable Obj Mgr Degug services if slub build
	CONFIG_WLAN_OBJMGR_DEBUG:= y
	CONFIG_LOCK_STATS_ON:= y
endif

ifeq (y,$(findstring y,$(CONFIG_QCA_WIFI_SDIO) $(CONFIG_HIF_USB)))
CONFIG_HL_DP_SUPPORT := y
else
CONFIG_LL_DP_SUPPORT := y
endif

ifeq ($(CONFIG_ROME_IF),pci)
ifneq ($(CONFIG_WLAN_TX_FLOW_CONTROL_V2), y)
ifneq ($(CONFIG_LITHIUM), y)
CONFIG_WLAN_TX_FLOW_CONTROL_LEGACY := y
endif
endif
endif

#Whether have QMI support
CONFIG_QMI_SUPPORT := y

ifeq ($(CONFIG_ICNSS), y)
CONFIG_WIFI_3_0_ADRASTEA := y
CONFIG_ADRASTEA_RRI_ON_DDR := y
# Enable athdiag procfs debug support for adrastea
CONFIG_ATH_PROCFS_DIAG_SUPPORT := y
# Enable 11AC TX compact feature for adrastea
CONFIG_ATH_11AC_TXCOMPACT := y
ifeq ($(CONFIG_QMI_SUPPORT), y)
CONFIG_ADRASTEA_SHADOW_REGISTERS := y
endif
endif

# Enable fw stats version 2
ifeq (y,$(findstring y,$(CONFIG_HELIUMPLUS) $(CONFIG_LITHIUM)))
CONFIG_AR900B := y
endif

# NOTE: CONFIG_64BIT_PADDR requires CONFIG_HELIUMPLUS
ifeq ($(CONFIG_HELIUMPLUS), y)

ifeq ($(CONFIG_64BIT_PADDR), y)
CONFIG_HTT_PADDR64 := y
endif

ifeq ($(CONFIG_SLUB_DEBUG_ON), y)
CONFIG_OL_RX_INDICATION_RECORD := y
CONFIG_TSOSEG_DEBUG := y
endif

endif #CONFIG_HELIUMPLUS

ifeq ($(CONFIG_LITHIUM), y)
#
# Enable Shadow V2 for all lithium platform
#
CONFIG_SHADOW_V2 := y

ifeq ($(CONFIG_CNSS_QCA6390), y)
	CONFIG_QCA6390_HEADERS_DEF := y
	CONFIG_QCA_WIFI_QCA6390 := y
endif

CONFIG_QCA_WIFI_QCA8074 := y
CONFIG_QCA_WIFI_QCA8074_VP := y
CONFIG_DP_INTR_POLL_BASED := y
CONFIG_TX_PER_PDEV_DESC_POOL := y
CONFIG_DP_TRACE := y
CONFIG_FEATURE_TSO := y
CONFIG_TSO_DEBUG_LOG_ENABLE := y
CONFIG_DP_LFR := y
CONFIG_HTT_PADDR64 := y
CONFIG_RX_OL := y
CONFIG_TX_TID_OVERRIDE := y
CONFIG_DP_TXRX_SOC_ATTACH := y
CONFIG_REO_DESC_DEFER_FREE := y
endif #CONFIG_LITHIUM

# As per target team, build is done as follows:
# Defconfig : build with default flags
# Slub      : defconfig  + CONFIG_SLUB_DEBUG=y +
#	      CONFIG_SLUB_DEBUG_ON=y + CONFIG_PAGE_POISONING=y
# Perf      : Using appropriate msmXXXX-perf_defconfig
#
# Shipment builds (user variants) should not have any debug feature
# enabled. This is identified using 'TARGET_BUILD_VARIANT'. Slub builds
# are identified using the CONFIG_SLUB_DEBUG_ON configuration. Since
# there is no other way to identify defconfig builds, QCOMs internal
# representation of perf builds (identified using the string 'perf'),
# is used to identify if the build is a slub or defconfig one. This
# way no critical debug feature will be enabled for perf and shipment
# builds. Other OEMs are also protected using the TARGET_BUILD_VARIANT
# config.
ifneq ($(TARGET_BUILD_VARIANT),user)
	ifeq ($(CONFIG_LITHIUM), y)
		CONFIG_FEATURE_PKTLOG := n
	else
		CONFIG_FEATURE_PKTLOG := y
	endif
	CONFIG_WLAN_DEBUG_CRASH_INJECT := y
endif

#Enable WLAN/Power debugfs feature only if debug_fs is enabled
ifeq ($(CONFIG_DEBUG_FS), y)
       # Flag to enable debugfs. Depends on CONFIG_DEBUG_FS in kernel
       # configuration.
       CONFIG_WLAN_DEBUGFS := y

       CONFIG_WLAN_POWER_DEBUGFS := y
ifeq ($(CONFIG_RELAY), y)
       CONFIG_WLAN_STREAMFS := y
endif
endif

#Whether to build debug version
CONFIG_WLAN_DEBUG_VERSION := y

#Enable this flag to build driver in diag version
CONFIG_WLAN_DIAG_VERSION := y

ifeq ($(CONFIG_SLUB_DEBUG), y)
	PANIC_ON_BUG := y
	WLAN_WARN_ON_ASSERT := y
else ifeq ($(CONFIG_PERF_DEBUG), y)
	PANIC_ON_BUG := y
	WLAN_WARN_ON_ASSERT := y
else
	PANIC_ON_BUG := n
	WLAN_WARN_ON_ASSERT := n
endif

# Compile all log levels by default
CONFIG_WLAN_LOG_FATAL := y
CONFIG_WLAN_LOG_ERROR := y
CONFIG_WLAN_LOG_WARN := y
CONFIG_WLAN_LOG_INFO := y
CONFIG_WLAN_LOG_DEBUG := y
CONFIG_WLAN_LOG_ENTER := y
CONFIG_WLAN_LOG_EXIT := y

#Enable OL debug and wmi unified functions
CONFIG_ATH_PERF_PWR_OFFLOAD := y

#Disable packet log
CONFIG_REMOVE_PKT_LOG := n

#Enable 11AC TX
ifeq ($(CONFIG_ROME_IF),pci)
	CONFIG_ATH_11AC_TXCOMPACT := y
endif

ifeq ($(CONFIG_ROME_IF),usb)
	CONFIG_ATH_11AC_TXCOMPACT := n
endif

#Enable PCI specific APIS (dma, etc)
ifeq ($(CONFIG_ROME_IF),pci)
	CONFIG_HIF_PCI := y
endif

#Enable USB specific APIS
ifeq ($(CONFIG_ROME_IF),usb)
	CONFIG_HIF_USB := y
endif

#Enable SDIO specific APIS
ifeq ($(CONFIG_ROME_IF),sdio)
	CONFIG_HIF_SDIO := y
	CONFIG_TX_DESC_HI_PRIO_RESERVE := y
	CONFIG_PER_VDEV_TX_DESC_POOL := y
	CONFIG_FEATURE_HL_GROUP_CREDIT_FLOW_CONTROL := y
endif

ifeq ($(CONFIG_ROME_IF),snoc)
	CONFIG_HIF_SNOC:= y
endif

# enable/disable feature flags based upon mobile router profile
ifeq ($(CONFIG_MOBILE_ROUTER), y)
CONFIG_FEATURE_WLAN_MCC_TO_SCC_SWITCH := y
CONFIG_FEATURE_WLAN_AUTO_SHUTDOWN := y
CONFIG_FEATURE_WLAN_AP_AP_ACS_OPTIMIZE := y
CONFIG_FEATURE_WLAN_STA_4ADDR_SCHEME := y
CONFIG_MDM_PLATFORM := y
CONFIG_FEATURE_WLAN_STA_AP_MODE_DFS_DISABLE := y
CONFIG_FEATURE_AP_MCC_CH_AVOIDANCE := y
else
CONFIG_QCOM_ESE := y
CONFIG_WLAN_OPEN_P2P_INTERFACE := y
CONFIG_WLAN_ENABLE_SOCIAL_CHANNELS_5G_ONLY := y
endif

#enable 4addr support for QCS405
ifeq ($(CONFIG_ARCH_QCS405), y)
CONFIG_FEATURE_WLAN_STA_4ADDR_SCHEME := y
endif

#Enable power management suspend/resume functionality to PCI
CONFIG_ATH_BUS_PM := y

#Enable FLOWMAC module support
CONFIG_ATH_SUPPORT_FLOWMAC_MODULE := n

#Enable spectral support
CONFIG_ATH_SUPPORT_SPECTRAL := n

#Enable WDI Event support
ifeq ($(CONFIG_REMOVE_PKT_LOG), y)
CONFIG_WDI_EVENT_ENABLE := n
else
CONFIG_WDI_EVENT_ENABLE := y
endif

#Enable the type_specific_data in the ath_pktlog_arg
ifeq ($(CONFIG_REMOVE_PKT_LOG), n)
CONFIG_PKTLOG_HAS_SPECIFIC_DATA := y
endif

#Endianness selection
CONFIG_LITTLE_ENDIAN := y

#Enable TX reclaim support
CONFIG_TX_CREDIT_RECLAIM_SUPPORT := n

#Enable FTM support
CONFIG_QCA_WIFI_FTM := y

ifeq ($(CONFIG_QCA_WIFI_FTM), y)

ifeq ($(CONFIG_NL80211_TESTMODE), y)
	QCA_WIFI_FTM_NL80211 :=y
else
	QCA_WIFI_FTM_NL80211 :=n
endif
	CONFIG_LINUX_QCMBR :=y

else
	QCA_WIFI_FTM_NL80211 :=n
	CONFIG_LINUX_QCMBR :=n
endif


#Enable Checksum Offload
CONFIG_CHECKSUM_OFFLOAD := y

#Enable GTK offload
CONFIG_GTK_OFFLOAD := y

#Set this to 1 to catch erroneous Target accesses during debug.
CONFIG_ATH_PCIE_ACCESS_DEBUG := n

#Enable IPA offload
ifeq ($(CONFIG_IPA), y)
CONFIG_IPA_OFFLOAD := y
endif
ifeq ($(CONFIG_IPA3), y)
CONFIG_IPA_OFFLOAD := y
endif

ifeq ($(CONFIG_IPA_OFFLOAD), y)
CONFIG_SMMU_S1_UNMAP := y
endif

#Flag to enable SMMU S1 support
ifeq ($(CONFIG_ARCH_SDM845), y)
ifeq ($(CONFIG_IPA_OFFLOAD), y)
CONFIG_ENABLE_SMMU_S1_TRANSLATION := y
endif
endif

ifeq ($(CONFIG_ARCH_SM8150), y)
ifeq ($(CONFIG_IPA_OFFLOAD), y)
CONFIG_ENABLE_SMMU_S1_TRANSLATION := y
endif
endif

#Flag to enable SMMU S1 support
ifeq (y, $(filter y, $(CONFIG_ARCH_SDXPRAIRIE) $(CONFIG_ARCH_SA515)))
ifeq ($(CONFIG_IPA_OFFLOAD), y)
CONFIG_ENABLE_SMMU_S1_TRANSLATION := y
endif
endif

ifeq ($(CONFIG_IPA_OFFLOAD), y)
CONFIG_IPA_P2P_SUPPORT := y
endif

ifeq ($(CONFIG_ARCH_SDX20), y)
ifeq ($(CONFIG_QCA_WIFI_SDIO), y)
ifeq ($(CONFIG_WCNSS_SKB_PRE_ALLOC), y)
CONFIG_FEATURE_SKB_PRE_ALLOC := y
endif
endif
endif

#Enable Signed firmware support for split binary format
CONFIG_QCA_SIGNED_SPLIT_BINARY_SUPPORT := n

#Enable single firmware binary format
CONFIG_QCA_SINGLE_BINARY_SUPPORT := n

#Enable collecting target RAM dump after kernel panic
CONFIG_TARGET_RAMDUMP_AFTER_KERNEL_PANIC := y

#Flag to enable/disable secure firmware feature
CONFIG_FEATURE_SECURE_FIRMWARE := n

#Flag to enable Stats Ext implementation
CONFIG_FEATURE_STATS_EXT := y

#Flag to allocate memory dynamically for different buffers
CONFIG_WLAN_LOGGING_BUFFERS_DYNAMICALLY := n
CONFIG_WLAN_DFS_STATIC_MEM_ALLOC := y

#Flag to enable HTC credit history feature
CONFIG_FEATURE_HTC_CREDIT_HISTORY := y

#Flag to enable MTRACE feature
CONFIG_TRACE_RECORD_FEATURE := y

#Flag to enable p2p debug feature
CONFIG_WLAN_FEATURE_P2P_DEBUG := y

#Flag to enable roam debug log
CONFIG_FEATURE_ROAM_DEBUG := y

#Flag to enable DFS Master feature
CONFIG_WLAN_DFS_MASTER_ENABLE := y

#Flag to enable WEXT support for STA/AP/P2P interfaces
ifeq ($(CONFIG_WIRELESS_EXT), y)
CONFIG_WLAN_WEXT_SUPPORT_ENABLE := y
endif

#Flag to enable/disable MTRACE feature
CONFIG_ENABLE_MTRACE_LOG := y

#Flag to enable nud tracking feature
CONFIG_WLAN_NUD_TRACKING := y

#Flag to enable wbuff feature
CONFIG_WLAN_WBUFF := y

#Flag to enable set and get disable channel list feature
CONFIG_DISABLE_CHANNEL_LIST :=y

#Flag to enable Dynamic Voltage WDCVS (Config Voltage Mode)
CONFIG_WLAN_DYNAMIC_CVM := y

CONFIG_WIFI_POS_CONVERGED := y
ifneq ($(CONFIG_WIFI_POS_CONVERGED), y)
CONFIG_WIFI_POS_LEGACY := y
endif

CONFIG_CP_STATS := y

#Flag to enable compilation of DCS module
CONFIG_DCS := y

CONFIG_FEATURE_WLAN_WAPI := y

CONFIG_AGEIE_ON_SCAN_RESULTS := y

#Flag to enable FW log parsing support feature
CONFIG_FEATURE_FW_LOG_PARSING := y

CONFIG_PTT_SOCK_SVC_ENABLE := y
CONFIG_SOFTAP_CHANNEL_RANGE := y
CONFIG_FEATURE_WLAN_SCAN_PNO := y
CONFIG_WLAN_FEATURE_PACKET_FILTERING := y
CONFIG_WLAN_NS_OFFLOAD := y
CONFIG_FEATURE_WLAN_RA_FILTERING:= y
CONFIG_FEATURE_WLAN_LPHB := y
CONFIG_QCA_SUPPORT_TX_THROTTLE := y
CONFIG_WMI_INTERFACE_EVENT_LOGGING := y
CONFIG_WLAN_FEATURE_LINK_LAYER_STATS := y
CONFIG_FEATURE_WLAN_EXTSCAN := n
CONFIG_WMI_BCN_OFFLOAD := y
CONFIG_160MHZ_SUPPORT := y
CONFIG_REG_CLIENT := y
CONFIG_WLAN_PMO_ENABLE := y
CONFIG_CONVERGED_P2P_ENABLE := y
CONFIG_WLAN_POLICY_MGR_ENABLE := y
CONFIG_FEATURE_DENYLIST_MGR := y
CONFIG_SUPPORT_11AX := y
CONFIG_HDD_INIT_WITH_RTNL_LOCK := y
CONFIG_WLAN_CONV_SPECTRAL_ENABLE := y
CONFIG_WLAN_SPECTRAL_ENABLE := y
CONFIG_WMI_CMD_STRINGS := y
CONFIG_FEATURE_MONITOR_MODE_SUPPORT := y
CONFIG_WLAN_ALLOCATE_GLOBAL_BUFFERS_DYNAMICALLY := n
CONFIG_WLAN_FEATURE_TWT := y

ifeq ($(CONFIG_WLAN_DEBUGFS), y)
       CONFIG_WLAN_FEATURE_MIB_STATS := y
endif

ifeq (y,$(findstring y,$(CONFIG_LITHIUM) $(CONFIG_ICNSS)))
CONFIG_WLAN_FEATURE_BMI := n
else
CONFIG_WLAN_FEATURE_BMI := y
endif

#Flags to enable/disable vendor commands
CONFIG_FEATURE_RSSI_MONITOR := y
CONFIG_FEATURE_BSS_TRANSITION := y
CONFIG_FEATURE_STATION_INFO := y
CONFIG_FEATURE_TX_POWER := y
CONFIG_FEATURE_OTA_TEST := y
CONFIG_FEATURE_ACTIVE_TOS := y
CONFIG_FEATURE_SAR_LIMITS := y
CONFIG_FEATURE_CONCURRENCY_MATRIX := y
CONFIG_FEATURE_SAP_COND_CHAN_SWITCH := y
CONFIG_FEATURE_P2P_LISTEN_OFFLOAD := y
CONFIG_QCACLD_RX_DESC_MULTI_PAGE_ALLOC := y

#Flags to enable/disable WMI APIs
CONFIG_WMI_ROAM_SUPPORT := y
CONFIG_WMI_CONCURRENCY_SUPPORT := y
CONFIG_WMI_STA_SUPPORT := y

#Flag to enable LTE COEX feature
CONFIG_LTE_COEX := y

#Flag to enable/disable TARGET 11d scan
CONFIG_TARGET_11D_SCAN := y

#Flag to enable HOST OPCLASS feature
CONFIG_HOST_OPCLASS := y

ifeq ($(CONFIG_HELIUMPLUS), y)
ifneq ($(CONFIG_FORCE_ALLOC_FROM_DMA_ZONE), y)
CONFIG_ENABLE_DEBUG_ADDRESS_MARKING := y
endif
CONFIG_RX_OL := y
endif

ifeq ($(CONFIG_SLUB_DEBUG_ON), y)
	CONFIG_DSC_DEBUG := y
	CONFIG_DESC_TIMESTAMP_DEBUG_INFO := y
	CONFIG_FEATURE_UNIT_TEST_SUSPEND := y
	CONFIG_LEAK_DETECTION := y
ifndef CONFIG_MAX_LOGS_PER_SEC
	CONFIG_MAX_LOGS_PER_SEC := 500
endif
	CONFIG_SCHED_HISTORY_SIZE := 256
	CONFIG_TALLOC_DEBUG := y
	CONFIG_UNIT_TEST := y
	CONFIG_HAL_DEBUG := y
endif

ifeq ($(CONFIG_UNIT_TEST), y)
	CONFIG_DSC_TEST := y
	CONFIG_QDF_TEST := y
endif

# enable unit-test suspend for napier builds
ifeq ($(CONFIG_LITHIUM), y)
	CONFIG_FEATURE_UNIT_TEST_SUSPEND := y
	CONFIG_FIX_TXDMA_LIMITATION := y
	CONFIG_FEATURE_AST := y
	CONFIG_PEER_PROTECTED_ACCESS := y
	CONFIG_SERIALIZE_QUEUE_SETUP := y
	CONFIG_DP_RX_PKT_NO_PEER_DELIVER := y
	CONFIG_DP_RX_DROP_RAW_FRM := y
	CONFIG_FEATURE_ALIGN_STATS_FROM_DP := y
	CONFIG_DP_RX_SPECIAL_FRAME_NEED := y
	CONFIG_FEATURE_STATS_EXT_V2 := y
	CONFIG_WLAN_FEATURE_DP_RX_THREADS := y
	CONFIG_WLAN_FEATURE_RX_SOFTIRQ_TIME_LIMIT := y
	CONFIG_FEATURE_NO_DBS_INTRABAND_MCC_SUPPORT := y
	CONFIG_HAL_DISABLE_NON_BA_2K_JUMP_ERROR := y
	CONFIG_ENABLE_HAL_SOC_STATS := y
	CONFIG_ENABLE_HAL_REG_WR_HISTORY := y
	CONFIG_MON_ENABLE_DROP_FOR_MAC := y
	CONFIG_PCI_LINK_STATUS_SANITY := y
	CONFIG_DDP_MON_RSSI_IN_DBM := y
	CONFIG_SYSTEM_PM_CHECK := y
	CONFIG_DISABLE_EAPOL_INTRABSS_FWD := y
endif

#Flag to enable hdd memory dump feature
CONFIG_FEATURE_MEMDUMP_ENABLE := y

#Flag to enable/disable WLAN D0-WOW
ifeq ($(CONFIG_PCI_MSM), y)
ifeq ($(CONFIG_HIF_PCI), y)
CONFIG_FEATURE_WLAN_D0WOW := y
endif
endif

ifeq ($(CONFIG_ARCH_MDM9607), y)
CONFIG_TUFELLO_DUAL_FW_SUPPORT := y
endif

ifeq ($(CONFIG_ARCH_MSM8996), y)
CONFIG_CHANNEL_HOPPING_ALL_BANDS := y
endif

ifeq (y, $(filter y, $(CONFIG_ARCH_SDXPRAIRIE) $(CONFIG_ARCH_SA515)))
	CONFIG_FEATURE_MONITOR_MODE_SUPPORT := n
	ifneq ($(CONFIG_SLUB_DEBUG), y)
		CONFIG_DP_TRACE := n
	endif
endif

ifneq ($(CONFIG_HIF_USB), y)
CONFIG_WLAN_LOGGING_SOCK_SVC := y
endif

ifneq ($(TARGET_BUILD_VARIANT),user)
CONFIG_DESC_DUP_DETECT_DEBUG := y
CONFIG_DEBUG_RX_RING_BUFFER := y
endif


ifeq ($(CONFIG_CNSS), y)
ifeq ($(CONFIG_CNSS_SDIO), y)
CONFIG_PLD_SDIO_CNSS_FLAG := y
endif
ifeq ($(CONFIG_HIF_PCI), y)
CONFIG_PLD_PCIE_CNSS_FLAG := y
endif
endif

ifeq ($(CONFIG_CNSS2), y)
ifeq ($(CONFIG_HIF_PCI), y)
CONFIG_PLD_PCIE_CNSS_FLAG := y
CONFIG_PLD_PCIE_INIT_FLAG := y
endif
endif

ifeq ($(CONFIG_CNSS2), m)
ifeq ($(CONFIG_HIF_PCI), y)
CONFIG_PLD_PCIE_CNSS_FLAG := y
CONFIG_PLD_PCIE_INIT_FLAG := y
endif
endif

#Enable STATE MACHINE HISTORY
CONFIG_SM_ENG_HIST := n

ifeq ($(CONFIG_WLAN_SYSFS), y)
#Enable Beacon Reception Stats
CONFIG_FEATURE_BECN_STATS := y
endif

ifeq (y,$(findstring y,$(CONFIG_ARCH_MSM) $(CONFIG_ARCH_QCOM)))
CONFIG_WLAN_FEATURE_DP_BUS_BANDWIDTH := y
endif

CONFIG_FOURTH_CONNECTION := y
CONFIG_FOURTH_CONNECTION_AUTO := y
CONFIG_SAP_DHCP_FW_IND := y

#Enable FW Offload
CONFIG_WLAN_FW_OFFLOAD := y

CONFIG_WLAN_FEATURE_MEDIUM_ASSESS := y

#Enable Usable channel feature
CONFIG_WLAN_FEATURE_GET_USABLE_CHAN_LIST := y

ifeq ($(CONFIG_MSM_BOOT_TIME_MARKER), y)
CONFIG_WLAN_BOOTUP_MARKER := y
endif

CONFIG_WLAN_SYSFS_MEM_STATS := y

CONFIG_WLAN_DP_PENDING_MEM_FLUSH := y

CONFIG_WLAN_TRACEPOINTS := y

ifeq ($(CONFIG_CNSS2), m)
CONFIG_CNSS2_MODULE := y
endif

ifeq ($(CONFIG_CNSS_GENL), m)
CONFIG_CNSS_GENL_MODULE := y
endif

ifeq ($(CONFIG_CNSS_UTILS), m)
CONFIG_CNSS_UTILS_MODULE := y
endif
